/* English error messages table,   Attention : en cas de rajout de messages, modifier l'enum de plpmsg.h */

	"Success",
	"Parameters error ",
	"Conversion parameters error: ",
	"Result parameters error: ",
	"Communication error with terminal",
	"Timeout reception with terminal response",
	"Timeout reception with terminal results",
	"Parameters error in the terminal response",
	"Returned error by the terminal",
	"Serial link is not open",
	"Inner error : primitives driver",
	"Inner error : product driver",
	"Inner error : messages administration",
	"Inner error : communication driver",
	"Inner error : absent file",
	"Inner error : downloading driver",
	"BBIC error : BC_OM_ERROR received",
	"EEPROM reading problem",
	"EEPROM writing problem",
	"EEPROM checksum update problem",
	"Problem with Flash Erasing",
	"Problem with Flash Writing",
	"Bsic not found",
	"Desinscription Bbase error",
	"Inscription Bbase error",
	"Synchro activation error",
	"The terminal is already connected",
	"The terminal is already disconnected",

/* Erreurs driver LCE */

	"LCE parameters error",
	"Sending message error to embedded router",
	"BBIC sending message error",
	"LCE sending message error",
	"LCE timeout reception message error",
	"LCE paramaters result error",

/* Erreurs driver communication */

	"Bad number of serial link",
	"Serial link opening error",
	"Serial link closing error",
	"Link initialization error",
	"Link closed error",
	"Change of configuration link error",
	"Serial link is already openned",
	"Serial link is already closed",
	"Serial port error",
	"MCX card error",
	"Sending message error",
	"Reception message error",
	"Communication Driver error",

/* Erreurs driver téléchargement */

	"Sending port error",
	"Reception port error",
	"Error : no more RAM available",
	
/* inserer ici les nouveaux messages */

